|  |  |  |
| --- | --- | --- |
| **Name of camp:** | **Activity/Area being assessed:** Aerial runway | **Camp leader’s name:** |
| **Name(s) of risk assessors** | **Date risk assessment undertaken:** 14/03/2023 | **Time period risk assessment is valid for:** One Year |

| **What are the hazards?** | **Who could be harmed and how?** | **What controls do you have in place?** | **Are further controls needed? Yes/No if yes please outline below** | **Date action completed** |
| --- | --- | --- | --- | --- |
| Aerial Runway | User  Injury | Aerial Runway Handbook outlines rules for safe use of runway.  No rider to be over 150kg.  User needs to be able to sit independently in chair – no doubling up on a helper’s lap.  Runway chair, straps and entire runway cables / ropes are serviced yearly prior to opening for the season.  First Aid Kit on site  Defib on site  Mobile Phones available to call emergency services if needed. | Operators to ensure guidelines are adhered to to ensure safe use. | When in use. |
| Descent too quick to landing area | User  Injury | Aerial Runway Handbook outlines rules for safe use of runway.  Responsible person to be at landing area and through radio or hand signals can communicate to operator to brake. | Controls to be operated by experienced / competent person.  Controller to ensure chair descends at low speed into landing bay using brake on controls. | When in use. |
| Runway chair hitting observer. | User / Other camp user  Injury | Aerial Runway Handbook outlines rules for safe use of runway.  Ride supervisors and bystanders instructed stand back from landing area. | Controller and base supervisor to be conversant with Handbook. | When in use. |
| Platform opened too soon / mechanism fails. | Users and helpers.  Injury | Aerial Runway Handbook outlines rules for safe use of runway.  Lights will show Green if platform is locked in place.  Gate to remain in place when loading and unloading. | Loaders to be conversant with Handbook.  Platform to be kept clear of bystanders | When in use |

**Signature of Risk Assessor:………………………… Print name…………………………………….. Date:…………………………………..**